1. Hubs broadcast data to all listening computers, while switches only transmit to intended for others. You can see others data using a hub.
2. I can’t see any on USC wifi
3. It is a service that allows for the transmission of voice data over wifi. There are several exploits of VoIP that exist. It is used by USC.